**Using the Microscope Fixes**

4. Revolve the nosepiece until the **scanning objective lens** clicks in place.

7. Carefully turn the coarse adjustment knob to lower the body tube until the **scanning objective is as low as it can get.**

9. Switch to **low power lens** by revolving the nosepiece until lens clicks into place. **You can use the coarse adjustment and fine adjustment knobs to focus on the specimen.**

10. Switch to the **high power lens** by revolving the nosepiece until the lens clicks into place. **You can only use the fine adjustment knob to focus on the specimen.**